{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["一标段","二标段","三标段"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"一标段","index":0,"n_rows":11,"n_cols":13,"rows_kept":11,"merged":[[0,0,0,12],[2,1,2,2],[5,0,5,2],[6,1,6,2],[7,0,7,10],[8,0,8,12]],"flags":["formulas_cached_only"]}
["盐城经济技术开发区东方集团软件园1#、4#楼电梯维护保养服务项目预算价"]
["序号","园区名称","电梯品牌种类","数量(台)","设备型号","层站","使用起始 年限","有无机房","维保起止时间","乘客电梯、货梯额定速度及自动扶梯提升高度","全费用单价           (元/台/年)","合价（元）","备注"]
["一","电梯维护保养费"]
[1,"软件园1、4#楼","三菱电梯",4,"MAXIEZ-CZ","15∕15",2011.06,"有","2026.1.1～2026.12.31","1.6m∕s",null,0]
[2,"软件园1、4#楼","三菱电梯",6,"MAXIEZ-CZ","16∕16",2011.06,"有","2026.1.1～2026.12.31","1.6m∕s",null,0]
["小计",null,null,10,"/","/","/","/","/","/","/",0]
["二","特种设备检验检测费用",null,10,{"$nulls":7},0]
["\t合     计",{"$nulls":10},0]
["说明：1、投标报价为半包（包工包料），投标报价是指按招标人提供的招标服务内容，进行电梯的维护保养服务而涵盖的所有费用，包括但不仅限于人工费、材料费、配件费[免费提供部分电梯零部件（单价500元及以下、轿厢照明、层门滑块、润滑油）]、资料费、仪器设备或机械使用费、电梯年检费、提供技术资料、技术服务、配合特种设备检验检测机构进行电梯的定期检验、管理费、利润、税金，同时还应充分考虑市场风险、国家政策性调整风险系数以及承担的义务、责任、风险等一切因素，并计入投标报价中。\n2、更换的零部件要求：在电梯维保期间均采用原电梯使用的品牌零部件，并在更换前经招标人确认。\n3、每月2次派持有《特种设备作业人员证》（作业项目：电梯作业）的维保人员对电梯进行清洁、润滑、调整和检查等日常维护或保养性工作。\n4、提供24小时全天候急修服务。"]
[null,"投标单位盖章："]
[null,"时间："]

{"sheet":"二标段","index":1,"n_rows":28,"n_cols":13,"rows_kept":28,"merged":[[0,0,0,12],[2,1,2,2],[22,0,22,2],[23,1,23,2],[24,0,24,10],[25,0,25,12]],"flags":["formulas_cached_only"]}
["东科城58台电梯日常维护、保养和急修等半包（包工包料）服务项目预算价"]
["序号","园区名称","电梯品牌种类","数量(台)","设备型号","层站","使用起始 年限","有无机房","维保起止时间","乘客电梯、货梯额定速度及自动扶梯提升高度","全费用单价           (元/台/年)","合价（元）","备注"]
["一","电梯维护保养费"]
[1,"东科城","迅达曳引驱动乘客电梯",2,"Schindler 5000","12/12","2024.1","有","2026.01.01-2026.12.31","1.75m∕s",null,{"v":0,"d":"0.00"}]
[2,"东科城","迅达曳引驱动乘客电梯",4,"Schindler 5000","7/7","2024.1","有","2026.01.01-2026.12.31","1.75m∕s",null,{"v":0,"d":"0.00"}]
[3,"东科城","迅达曳引驱动乘客电梯",2,"Schindler 5000","7/7","2024.1","有","2026.01.01-2026.12.31","1.75m∕s",null,{"v":0,"d":"0.00"}]
[4,"东科城","迅达曳引驱动乘客电梯",14,"Schindler 5000","4/4","2024.1","有","2026.01.01-2026.12.31","1.75m∕s",null,{"v":0,"d":"0.00"}]
[5,"东科城","迅达曳引驱动乘客电梯",6,"Schindler 5000","16/16","2024.1","有","2026.01.01-2026.12.31","1.75m∕s",null,{"v":0,"d":"0.00"}]
[6,"东科城","迅达曳引驱动乘客电梯",2,"Schindler 5000","4/4","2024.1","有","2026.01.01-2026.12.31","1.75m∕s",null,{"v":0,"d":"0.00"}]
[7,"东科城","迅达曳引驱动乘客电梯",2,"Schindler 5000","4/4","2024.1","无","2026.01.01-2026.12.31","1.75m∕s",null,{"v":0,"d":"0.00"}]
[8,"东科城","迅达曳引驱动乘客电梯",1,"Schindler 5000","12/12","2024.1","有","2026.01.01-2026.12.31","1.75m∕s",null,{"v":0,"d":"0.00"}]
[9,"东科城","迅达曳引驱动乘客电梯",2,"Schindler 5000","7/7","2024.1","有","2026.01.01-2026.12.31","1.75m∕s",null,{"v":0,"d":"0.00"}]
[10,"东科城","迅达曳引驱动乘客电梯",2,"Schindler 5000","12/12","2024.1","有","2026.01.01-2026.12.31","1.75m∕s",null,{"v":0,"d":"0.00"}]
[11,"东科城","迅达曳引驱动乘客电梯",1,"Schindler 5000","16/16","2024.1","有","2026.01.01-2026.12.31","1.75m∕s",null,{"v":0,"d":"0.00"}]
[12,"东科城","迅达曳引驱动乘客电梯",3,"Schindler 5000","14/14","2024.1","有","2026.01.01-2026.12.31","1.75m∕s",null,{"v":0,"d":"0.00"}]
[13,"东科城","迅达曳引驱动乘客电梯",1,"Schindler 5000","14/14","2024.1","有","2026.01.01-2026.12.31","1.75m∕s",null,{"v":0,"d":"0.00"}]
[14,"东科城","迅达曳引驱动乘客电梯",1,"Schindler 5000","16/16","2024.1","有","2026.01.01-2026.12.31","1.75m∕s",null,{"v":0,"d":"0.00"}]
[15,"东科城","迅达曳引驱动乘客电梯",1,"Schindler 5000","16/16","2024.1","有","2026.01.01-2026.12.31","1.75m∕s",null,{"v":0,"d":"0.00"}]
[16,"东科城","迅达曳引驱动乘客电梯",2,"Schindler 5000","12/12","2024.1","有","2026.01.01-2026.12.31","1.75m∕s",null,{"v":0,"d":"0.00"}]
[17,"东科城","迅达曳引驱动乘客电梯",2,"Schindler 5000","7/7","2024.1","有","2026.01.01-2026.12.31","1.75m∕s",null,{"v":0,"d":"0.00"}]
[18,"东科城","菱王曳引驱动载货电梯",6,"LTHW","4/4",2023.11,"有","2026.01.01-2026.12.31","0.5m∕s",null,{"v":0,"d":"0.00"}]
[19,"东科城","江南嘉捷扶梯",4,"KNB4170","2/2",2024.11,"有","2026.01.20-2026.12.31","0.6m∕s",null,{"v":0,"d":"0.00"}]
["小计",null,null,58,"/","/","/","/","/","/","/",0]
["二","特种设备检验检测费用",null,58,{"$nulls":7},0]
["\t合     计",{"$nulls":10},0]
["说明：1、投标报价为半包（包工包料），投标报价是指按招标人提供的招标服务内容，进行电梯的维护保养服务而涵盖的所有费用，包括但不仅限于人工费、材料费、配件费[免费提供部分电梯零部件（单价500元及以下、轿厢照明、层门滑块、润滑油）]、资料费、仪器设备或机械使用费、电梯年检费、提供技术资料、技术服务、配合特种设备检验检测机构进行电梯的定期检验、管理费、利润、税金，同时还应充分考虑市场风险、国家政策性调整风险系数以及承担的义务、责任、风险等一切因素，并计入投标报价中。\n2、更换的零部件要求：在电梯维保期间均采用原电梯使用的品牌零部件，并在更换前经招标人确认。\n3、每月2次派持有《特种设备作业人员证》（作业项目：电梯作业）的维保人员对电梯进行清洁、润滑、调整和检查等日常维护或保养性工作。\n4、提供24小时全天候急修服务。"]
[null,"投标单位盖章："]
[null,"时间："]

{"sheet":"三标段","index":2,"n_rows":19,"n_cols":13,"rows_kept":19,"merged":[[0,0,0,12],[2,1,2,2],[13,0,13,2],[14,1,14,2],[15,0,15,10],[16,0,16,12]],"flags":["formulas_cached_only"]}
["盐城经济技术开发区漕河泾园区电梯维护保养服务项目预算价"]
["序号","园区名称","电梯品牌种类","数量(台)","设备型号","层站","使用起始 年限","有无机房","维保起止时间","乘客电梯、货梯额定速度及自动扶梯提升高度","全费用单价           (元/台/年)","合价（元）","备注"]
["一","电梯维护保养费"]
[1,"漕河泾园区研发楼","日立曳引驱动乘客电梯",3,"UAX-1000-C090","5∕4",2012.09,"有","2026.1.1～2026.12.31","1.5m∕s",null,0]
[2,"漕河泾园区研发楼","日立曳引驱动乘客电梯",1,"UAX-1000-C090","5∕5",2012.09,"有","2026.1.1～2026.12.31","1.5m∕s",null,0]
[3,"漕河泾园区2A楼","凯斯博曳引驱动乘客电梯",1,"KA-MRL000Ｘ100EIC","5∕5",2015.06,"有","2026.1.1～2026.12.31","1.0m∕s",null,0]
[4,"漕河泾园区2A楼","凯斯博曳引驱动乘客电梯",1,"KA-FG1250Ｘ100EIC","5∕5",2015.06,"有","2026.1.1～2026.12.31","1.0m∕s",null,0]
[5,"漕河泾园区2B楼","凯斯博曳引驱动载货电梯",1,"KA-FG1250Ｘ50EIC","5∕5",2014.04,"有","2026.1.1～2026.12.31","0.5m∕s",null,0]
[6,"漕河泾园区2B楼","凯斯博曳引驱动乘客电梯",1,"KA-MRL000Ｘ100EIC","5∕5",2014.04,"有","2026.1.1～2026.12.31","1.0m∕s",null,0]
[7,"漕河泾园区4A楼","西继迅达曳引驱动乘客电梯",2,"9000-WT-10-10-2-XS","4∕4",2013.11,"有","2026.1.1～2026.12.31","1.0m∕s",null,0]
[8,"漕河泾园区4B楼","广东快速曳引驱动乘客电梯",2,"TK(W)1000/1.0-JX.VF","5∕5",2015.01,"有","2026.1.1～2026.12.31","1.0m∕s",null,0]
[9,"漕河泾园区5A楼","奥克斯快速曳引驱动乘客电梯",2,"APN（1000/1.0JXW）","4∕4",2014.08,"有","2026.1.1～2026.12.31","1.0m∕s",null,0]
[10,"漕河泾园区5B楼","奥克斯快速曳引驱动乘客电梯",2,"APN（1000/1.0JXW）","5∕5",2014.08,"有","2026.1.1～2026.12.31","1.0m∕s",null,0]
["小计",null,null,16,"/","/","/","/","/","/","/",0]
["二","特种设备检验检测费用",null,16,{"$nulls":7},0]
["\t合     计",{"$nulls":10},0]
["说明：1、投标报价为半包（包工包料），投标报价是指按招标人提供的招标服务内容，进行电梯的维护保养服务而涵盖的所有费用，包括但不仅限于人工费、材料费、配件费[免费提供部分电梯零部件（单价500元及以下、轿厢照明、层门滑块、润滑油）]、资料费、仪器设备或机械使用费、电梯年检费、提供技术资料、技术服务、配合特种设备检验检测机构进行电梯的定期检验、管理费、利润、税金，同时还应充分考虑市场风险、国家政策性调整风险系数以及承担的义务、责任、风险等一切因素，并计入投标报价中。\n2、更换的零部件要求：在电梯维保期间均采用原电梯使用的品牌零部件，并在更换前经招标人确认。\n3、每月2次派持有《特种设备作业人员证》（作业项目：电梯作业）的维保人员对电梯进行清洁、润滑、调整和检查等日常维护或保养性工作。\n4、提供24小时全天候急修服务。"]
[null,"投标单位盖章："]
[null,"时间："]